10-Port Oxygen Flow Meter for Live Fish Transport Vehicles
Product Overview
The 10-Port Oxygen Flowmeter is a compact and efficient distribution system that supplies both pure and emergency oxygen from an oxygen generator to each tank in a live fish transport vehicle. Designed at half the size of conventional models, it optimizes installation space while maintaining high performance.
Even in the event of a leak in one tank, the system’s independent channel design minimizes any impact on other tanks, ensuring stable oxygen delivery throughout. Each port is equipped with a 3L fine-adjustable flowmeter, allowing precise control of oxygen flow for optimal live fish health and transport conditions.
Key Features:
· 10 independent oxygen supply ports
· Compact design (approximately 50% smaller than standard units)
· Leak-isolation structure for system stability
· 3L precision flow adjustment for each port
· Ideal for live fish transport and aquaculture applications
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Product Specification
	Category
	Specification

	Product Name
	Flowmeter (10 Ports)

	Model Name
	O2MOS-3L-10LINE-FM

	Component
	Main body, 10 × 3L Flowmeters, 4bar Gauge, 10-Port Manifold, Fittings

	Flow Rate Display
	0 ~ 3 LPM

	Oxygen Inlet Line
	Ø6 mm One-touch fitting (attached outside box)

	Oxygen Outlet Line
	Ø0.8 mm PVC nipple connection

	Dimensions / Weight
	600 × 120 × 200 mm / 5 kg

	Material
	STS304




Installation & Wiring Instructions
L-shaped body with multiple screw holes at the bottom for secure mounting
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