4-Port Oxygen Flow Meter for Live Fish Transport Vehicles
Product Overview
The 4-Port Oxygen Flow Meter efficiently distributes pure oxygen and emergency oxygen from an oxygen generator to multiple tanks in a live fish transport vehicle. Designed for performance and compactness, it is about half the size of conventional models, making installation and maintenance more convenient.
A key feature of this system is its independent flow design, which minimizes the impact on other tanks even if a leakage occurs in one tank, ensuring stable oxygen supply and fish safety. Each port is equipped with a 3L precision flow meter, allowing fine and accurate oxygen control for each tank.
Key Features:
· 4-port oxygen distribution system for live fish transport vehicles
· Supplies both pure and emergency oxygen from the generator
· Compact design — approximately 50% smaller than conventional models
· Independent flow structure minimizes inter-tank impact in case of leakage
· Equipped with 3L precision flow meters for fine adjustment
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Product Specifications
	Category
	Specification

	Product Name
	Flow Meter (4-Port)

	Model Name
	O2MOS-3L-4LINE-FM

	Device Components
	Main body, four 3L flow meters, 4 bar pressure gauge, 4-port manifold, fittings

	Flow Rate Display
	0 ~ 3 LPM

	Oxygen Inlet Line
	6mm one-touch fitting connection (attached to outer box casing)

	Oxygen Supply Line
	8mm PVC nipple

	Dimensions (mm) / Weight
	120 × 150 × 120 / 1.2Kg

	Material
	STS304
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