Driver-Side Oxygen Generator Controller 
Product Overview
The Vehicle Oxygen Generator Controller enables the driver to operate and monitor the PSA oxygen generator directly from the driver’s seat.
This control unit allows remote ON/OFF operation, real-time monitoring of the machine’s operating status, and oxygen supply condition through an intuitive interface.
By integrating the generator’s control and status monitoring into the vehicle dashboard, the system enhances user convenience, safety, and operational efficiency during transport and field operations.
Key Features:
· Remote ON/OFF control of the PSA oxygen generator from the driver’s seat
· Real-time display of machine operating status and oxygen supply level
· Compact and durable design suitable for vehicle installation
· Improves operational safety and ease of use during oxygen supply in mobile environments
· Alarm activates upon abnormal condition detection
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Product Specification
	Category
	Specification

	Product Name
	Driver-Side Controller

	Model Name
	O2MOS-CARCONTL-V1

	Control Method & Functions
	• Power supplied from oxygen generator part
• ON/OFF control of oxygen generator
• Monitoring operation status and oxygen delivery status
• Recording and storing usage time and method

	Connection
	4-pin for Power and Control

	Display
	Voltage, Oxygen Line Pressure, Normal operation Status

	Communication
	RS-485

	Dimensions 
	130 × 35 × 80 mm 

	Weight
	200g

	Housing Material
	Plastic



Installation & Wiring Instructions
• Installed on the driver’s side using bracket screws or double-sided tape
• Control cable routed from driver’s side to oxygen generator
• Protective tubing used for control cables

Ordering Information
O2MOS-12VC2-3LB2  : 3LPM, Vehicle-Mounted Oxygen Generator (12V)
O2MOS-24VC2-3LB2  : 3LPM, Vehicle-Mounted Oxygen Generator (24V)
O2MOS-12VC1-7LB2  :7LPM,  Vehicle-Mounted Oxygen Generator (12V)
O2MOS-24VC1-7LB1  : Vehicle-Mounted Oxygen Generator (24V)
O2MOS-CARCONTROL-V1 : Driver-Side controller
O2MOS-RO2S-SNL : Emergency Oxygen Alarm Device(Single)
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